COMMUNICATION & CONTROL PLENUM-RATED MULTIPAIR, INDIVIDUALLY FOIL SHIELDED FEP/PLENUM RATED

UL STANDARD 13, TYPE CL2P CSA PCC FT6 150 VOLT

APPLICATIONS

Remote Control Intercom Systems Burglar Alarm Systems Signaling And Power-Limited Circuits Cash Registers Other Low Voltage Systems

CHARACTERISTICS Operating Temperature:

-55ºC to 125ºC

Voltage Rating:

150 Volt

Color Desciption:

Color Code: See Chart Below Jacket Color: Gray

Product Description:

Conductor: Stranded Tinned Copper Shield: Each Pair Shielded With Aluminum Polyester Foil Insulation: Color-Coded FEP Drain Wire: Stranded Tinned Copper Jacket: Polyvinylidene Flouride (PVDF)

SPECIFICATIONS

UL Standard 13, Type CL2P CSA PCC FT6 Passes Steiner Tunnel Test

Passes Steiner Tunnel Test

AVAILABILITY

1000 ft (305m), 500 ft (152m) ^1000 ft (305m) 1000 ft put-ups may contain multiple lengths

Insulation Thickness: 0.007" (0,18mm)

Alpha Part No. No. of Pairs

Cond. AWG Size

Stranding Jacket Thickness In. mm

Diameter In. mm

Nominal Capacitance pF/ft

^58602
 58603
 58604
 58612*
 58613*
 58616*
 58632*
 58633
 58642
^58643

               2
               3
               4
               2
               3
               6
               2
               3
               2
               3

                     24
                     24
                     24
                     22
                     22
                     22
                     18
                     18
                     16
                     16

                               7/32
                               7/32
                               7/30
                               7/30
                               7/30
                               7/30
                           7/0.0152
                           7/0.0152
                           7/0.0192
                           7/0.0192

                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012
                                       0.012

                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30
                                               0,30

                                                       0.170
                                                       0.180
                                                       0.200
                                                       0.200
                                                       0.210
                                                       0.270
                                                       0.260
                                                       0.270
                                                       0.300
                                                       0.320

                                                                 4,3
                                                                 4,6
                                                                 5,1
                                                                 5,1
                                                                 5,3
                                                                 6,9
                                                                 6,7
                                                                 6,9
                                                                 7,6
                                                                 8,1

                                                                          25.2
                                                                          25.2
                                                                          25.2
                                                                          28.6
                                                                          28.6
                                                                          28.6
                                                                          35.5
                                                                          35.5
                                                                            38
                                                                            38

*These part numbers also have an overall aluminum/polyester shield

COLOR CODE CHART

Pair No. Combination

1 Black paired with Red

2 Black paired with White

3 Black paired with Green

4 Black paired with Blue

5 Black paired with Yellow

6 Black paired with Brown

Tel: 908-925-8000 Toll-Free: 1-800-52 ALPHA Fax: 908-925-6923

IN EUROPE: Tel: +44 01932 772422 Fax: +44 01932 772433

Master Catalog Page

223

Communication and Control Product Section Index

Who is Alpha - Online Catalog - Product Info/Search - Technical Info Marketing & Media - Ordering Info - Contact Us - Distributor Locator - Site Map

Copyright © 1998 Alpha Wire Company. All rights reserved.