A

A

B

B

C

C

D

D

E

E

F

F

G

G

H

H

I

I

J

J

1 1

2 2

3 3

4 4

5 5

6 6

7 7

Size: A No: Rev: 11

Sheet: 1 of 1 Revised: 20-Jan-2000

Drawn by: Created: 02-Dec-1999

File: c:\tw32demo\circuits\pulse.sch

RCVR

ARCNET

RCVR

GLINK

OPTO ISOL

OPTO ISOL.

8 BIT

SHIFT REG.

PULSE

+ DELAY GEN

8 BIT

10V DAC

ANALOG

SWITCH

10V

REFERENCE

ANALOG

SWITCHES

50 OHM

DRIVER

50 OHM

DRIVERs

Digital Power

+5VDC

+5VDC

+5VDC

+12VDC

+12VDC

Analog Power

+12VDC

+12VDC +12VDC

+12VDC

+12VDC

-12VDC

-12VDC

OR GATE

+12VDC

BUFFER

LEDs

FILTER

LOW PASS

MON

DAC OUT

MON

DRIVER OUT

RF OUT

1:2

TRANSFORMER

1:2

TRANSFORMERS

V1 +12VDC

V2 +5VDC X12 X10

0-10V

TRIGGER

ENABLE

GATE

X72

PULSE

ENABLE

PWR DOWN

Pulse into 100 Ohm

0-10V DIFF. X72

FIBER

UTP

TTL

OPTO ISOLATORS - TLP2200 (13) Toshiba

SHIFT REGISTERS - 74C164N (10) Fairchild

DAC + REFERENCE - AD7224LN + AD584JN Analog

PULSE GENERATOR - 74C221N Fairchild

QUAD ANALOG SWITCH - 74HC4066N (19) Fairchild

50 OHM DRIVER - AD8016 ARB (36) Analog

PULSE TRANSFORMER -

X2

X12

X8

T2.5-6-KK81 (72) Minicircuits (125 OHM)

18X4 36X2 72

9X4

QUAD OR GATE- 74C32N (18) Fairchild

POWER - +5V 2A, +12V 2A, -12V 2A

9X1

PULSE DRIVER ACTIVE

X72

OCTAL INVERTING BUFFER 74C240N (9) Fairchild

5V RESISTOR LED (72) Optrex

PULSE into 100 Ohm