2nd fiber pure silicon core fiber Fujikura sc 200/250,core f200m mcrad f250m mN.A. = 0.2length 40+5cm -0cm

Laser splitter

Start Counter

Beam expander

Wave length 355nm (THG)pulse width 30psEnergy/pulse 0.1mJ @355nm

YAG Laser1st Fiber Bundle2nd Fiber BundleTOF slat

Filtersdiffuser

1st fiber pure silicon core fiber Fujikura sc 600/750core f600m m/ crad f750m mN.A. = 0.2

37 1st fibers37 2nd fibers bundle f5mmbundle f1.5mmbeam f3mmbeam f25mm

Test Set Upobject linereferance line 123