Muon Workshop

M. Brooks 24-Oct-97

General μTr Soft ware St at us

PISORP code current ly cont ains: Turn (x,y) hit s int o charge on cat hodes/ anodes (use Landau for t ot al charge, Mat hieson for st rip dist ribut ion) Add noise t o st rips/ wires Apply t hresholds Find clust ers of hit st rips Fit clust ers t o Mat hieson dist ribut ions t o get measured cent roids (fit mult iple peaks if clust er widt h indicat es it should be) Degrade resolut ion for Lorent z angle, incident angle, st rip angle Find C-A-C clust ers Ret rieve hit s from a given t rack t hat form C-A-C clust ers Fit hit s t o get t rack t raject ory, moment um